Danú Channel List	

Ch. No.			Type			Instrument	
							
1			D.I(Compressor 1)	Bouzouki	
2			SM 58			Chat	
							
3			AKG 535(Compressor 2)	Flute	
							
4			D.I(Compressor 3)	Fiddle 	
5			SM 58			Chat/Harmony Vocals	
							
6			Beta SM 58(Compressor 4)	Lead Vocals	
							
7			SM 57(Compressor 5)	Button Accordion(High) 	
8			XLR			Button Accordion(Low)	
9			SM 58			Chat	
							
10			XLR			Pipes (High End)	
11			SM 57(Compressor 6)	Bodhran(Drum)	

12			DI(Compressor 7)		Guitar	
13			SM 58			Chat/Harmony Vocals	

The Desk
The mixing Desk must have the following
-24 channels(All with option of phantom power)
-2 sweepable mid EQ’s on each channel and a high pass filter
-4 pre-sends(Unless Onstage monitor mix is provided)
-At least 2 Post-sends(Reverb and Delay)
Example of Desk’s models-Midas,Crest,Dda,Yamaha,Allen & Heath and Soundcraft range.

NOTE- DIGITAL DESKS NOT ACCEPTED.

The Monitors
The following is required for on-stage monitors
-8 Monitor wedges of same design
-A minimum of 4 monitor mixes.
-31 band graphic EQ on each monitor mix.

Example of monitors-Eaw and Meyer

The Outboard Equipment
The outboard equipment should include the following
-2 Quality Progammable reverb units.
-1 Programmable delay unit.
-7 compressors.
-31 band front of house graphic’s

Note-Where monitors are controlled from front of house,the monitor graphics should be positioned beside the front of house desk,

The PA system(Must be in Stereo)
The PA must be
-Of professional quality.
-capable of  of producing 110 Db’s of full range sound without distortion at front of house mixing position. 
-Full range and controlled by active 3 way cross-overs and 31 band EQ’s Left and Right
 
Example of PA systems-EAW,MEYER,UPA,EV-DeltaMax or equivalent.

NOTE-IDEAL MIXING LOCATION IS THE CENTER OF THE VENUE.